IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2017-11-17T16:34:00"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1510936440 (2017-11-17T16:34:00Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1510936440 (2017-11-17T16:34:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "NBS_ARDEXUKLtd_HighPerformanceReadyMixedAdhesives_ARDEXAF200Plus_3mm" | FLOOR | names: "NBS_ARDEXUKLtd_HighPerformanceReadyMixedAdhesives_ARDEXAF200Plus_3mm" | material: layers "NBS_ARDEXUKLtd_HighPerformanceReadyMixedAdhesives_ARDEXAF200Plus_3mm" ("NBS_ARDEXUKLtd_HighPerformanceReadyMixedAdhesives_ARDEXAF200Plus_3mm" 3.) | property sets: COBie

Types
  IFCSLABTYPE "NBS_ARDEXUKLtd_HighPerformanceReadyMixedAdhesives_ARDEXAF200Plus_3mm" | FLOOR | 1 occurrence | material: layers "NBS_ARDEXUKLtd_HighPerformanceReadyMixedAdhesives_ARDEXAF200Plus_3mm" ("NBS_ARDEXUKLtd_HighPerformanceReadyMixedAdhesives_ARDEXAF200Plus_3mm" 3.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, NBS_General, NBS_Data, IFC

Property sets
  COBie | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_20_31_02_38:High-performance ready-mixed adhesives" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Uncoupling matting adhesive" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Significantly reduces the time required to install uncoupling mats prior to tiling; Suitable for adhering fleece-backed uncoupling matting to floors; High grab formulation reduces curling of the mat for easy installation; Ready to receive matting in as little as 5 minutes; Exceptionally long tack time allows matting to be fixed up to an hour after application; Once matting is installed, tiles can be fixed immediately; Priming rarely required; Ready mixed & resealable; Up to 45 m² coverage from a single tub; Solvent free, low odour & very low emissions" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@ardex.co.uk" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "ARDEX AF 200 Plus" (IFCTEXT)
    Name = "HighPerformanceReadyMixedAdhesives_ARDEXAF200Plus_ARDEXUKLtd" (IFCTEXT)
    NominalHeight = 3. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  xbim_MaterialFunctionAssignment | properties | on 1 type object
    MaterialFunctionAssignment (ifcpropertytablevalue)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "n/a" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 3. (IFCLENGTHMEASURE) [MILLI METRE]
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_ARDEXUKLtd_HighPerformanceReadyMixedAdhesives_ARDEXAF200Plus_3mm" (IFCTEXT)
    ManufacturerName = "ARDEX UK Ltd" (IFCTEXT)
    ManufacturerURL = "www.ardex.co.uk" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/i542xr1n" (IFCTEXT)
    NBSDescription = "High performance, ready mixed adhesives" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-50-00/435" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.ardex.co.uk/Portals/0/productdocs/7ce5cdb3-da6c-453c-a6c2-8500e230946d-ARDEX%20AF%20200%20PLUS.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_20_31_02_38" (IFCTEXT)
    Uniclass2015Title = "High-performance ready-mixed adhesives" (IFCTEXT)
    Uniclass2015Version = "Products v1.7" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Class = "n/a" (IFCTEXT)
    DryingTime = "n/a" (IFCTEXT)
    Fungicide = "n/a" (IFCTEXT)
    ShearAdhesionStrength = "n/a" (IFCTEXT)
    ShelfLife = "12 months" (IFCTEXT)
    SlumpResistance = "n/a" (IFCTEXT)
    TotalThicknessOptions = "n/a" (IFCTEXT)
    TotalVOCsMaximum = "n/a" (IFCTEXT)
  IFC | properties | on 1 type object
    IfcExportAs = "IfcCoveringType" (IFCTEXT)
    IfcExportType = "USERDEFINED" (IFCTEXT)