IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2017-11-17T16:33:59"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1510936439 (2017-11-17T16:33:59Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1510936439 (2017-11-17T16:33:59Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "NBS_ARDEXUKLtd_PolymerModifiedCementitiousMortar_ARDEXX7RW_1mm" | FLOOR | names: "NBS_ARDEXUKLtd_PolymerModifiedCementitiousMortar_ARDEXX7RW_1mm" | material: layers "NBS_ARDEXUKLtd_PolymerModifiedCementitiousMortar_ARDEXX7RW_1mm" ("NBS_ARDEXUKLtd_PolymerModifiedCementitiousMortar_ARDEXX7RW_1mm" 1.) | property sets: COBie

Types
  IFCSLABTYPE "NBS_ARDEXUKLtd_PolymerModifiedCementitiousMortar_ARDEXX7RW_1mm" | FLOOR | 1 occurrence | material: layers "NBS_ARDEXUKLtd_PolymerModifiedCementitiousMortar_ARDEXX7RW_1mm" ("NBS_ARDEXUKLtd_PolymerModifiedCementitiousMortar_ARDEXX7RW_1mm" 1.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, NBS_Data, NBS_General, IFC

Property sets
  COBie | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_20_31_53_65:Polymer-modified cementitious mortars" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Rapid setting flexible tile adhesive" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Walk on and grout tiles after 2 hours; Semi-pourable consistency, ideal for solid bed fixing large format floor tiles; Water content can be adjusted to produce a slump-free mix for coving/skirting and wall tiles; For use with all types of ceramic and porcelain tiles; Can be used on plywood overlay; Suitable for use with underfloor heating; For internal and external applications," (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@ardex.co.uk" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "ARDEX X 7 R W" (IFCTEXT)
    Name = "PolymerModifiedCementitiousMortar_ARDEXX7RW_1mm_ARDEXUKLtd" (IFCTEXT)
    NominalHeight = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  xbim_MaterialFunctionAssignment | properties | on 1 type object
    MaterialFunctionAssignment (ifcpropertytablevalue)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Cementitious adhesive" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  NBS_Data | properties | on 1 type object
    AdjustmentTime = "Approximately 20 mins" (IFCTEXT)
    BallPressureHardness = "n/a" (IFCTEXT)
    BulkDensityPowder = "n/a" (IFCTEXT)
    CompressiveStrength = "n/a" (IFCTEXT)
    FixingTime = "n/a" (IFCTEXT)
    SetFinal = "n/a" (IFCTEXT)
    SetInitial = "n/a" (IFCTEXT)
    ShelfLife = "12 months" (IFCTEXT)
    SlumpResistance = "Slip - less than 0.5mm" (IFCTEXT)
    TensileAdhesionStrength = "28 days dry: 1.0 N/mm², 28 days wet: 1.0 N/mm², After Freeze-Thaw: 1.0 N/mm², 24 hours dry: 0.5 N/mm²" (IFCTEXT)
    TensileBendingStrength = "n/a" (IFCTEXT)
    ThirdPartyProductCertification = "n/a" (IFCTEXT)
    TotalThicknessOptions = "n/a" (IFCTEXT)
    UnderflooringHeatingSuitablity = "Yes" (IFCTEXT)
    Walkability = "n/a" (IFCTEXT)
    WeightMortar = "Approximately 1.75kg/litre" (IFCTEXT)
    WorkingTime = "Approximately 30 mins" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_ARDEXUKLtd_PolymerModifiedCementitiousMortar_ARDEXX7RW_1mm" (IFCTEXT)
    ManufacturerName = "ARDEX UK Ltd" (IFCTEXT)
    ManufacturerURL = "www.ardex.co.uk" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/0njf0g5q" (IFCTEXT)
    NBSDescription = "Polymer-modified cementitious mortar" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-55-50/345" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.ardex.co.uk/Portals/0/productdocs/dfe26e0a-a6a6-4406-bc5c-357b91e27a4b-ARDEX%20X%207%20R%20Technical%20Datasheet.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_20_31_53_65" (IFCTEXT)
    Uniclass2015Title = "Polymer-modified cementitious mortars" (IFCTEXT)
    Uniclass2015Version = "Products v1.7" (IFCTEXT)
    Version = "1" (IFCTEXT)
  IFC | properties | on 1 type object
    IfcExportAs = "IfcCoveringType" (IFCTEXT)
    IfcExportType = "USERDEFINED" (IFCTEXT)