IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2017-11-17T16:33:52"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1510936432 (2017-11-17T16:33:52Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1510936432 (2017-11-17T16:33:52Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "NBS_ARDEXUKLtd_CementitiousAdhesives_ARDEXX7W_3mm" | FLOOR | names: "NBS_ARDEXUKLtd_CementitiousAdhesives_ARDEXX7W_3mm" | material: layers "NBS_ARDEXUKLtd_CementitiousAdhesives_ARDEXX7W_3mm" ("NBS_ARDEXUKLtd_CementitiousAdhesives_ARDEXX7W_3mm" 3.) | property sets: COBie

Types
  IFCSLABTYPE "NBS_ARDEXUKLtd_CementitiousAdhesives_ARDEXX7W_3mm" | FLOOR | 1 occurrence | material: layers "NBS_ARDEXUKLtd_CementitiousAdhesives_ARDEXX7W_3mm" ("NBS_ARDEXUKLtd_CementitiousAdhesives_ARDEXX7W_3mm" 3.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, NBS_General, NBS_Data, IFC

Property sets
  COBie | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_20_31_02_12:Cementitious adhesives" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "White tile adhesive with built-in admix" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Versatile multipurpose tile adhesives for fixing wall and floor tiles; Suitable for ceramic, porcelain, glass mosaic, and most natural stone tiles; For internal and external use; Frost and weather resistant; Suitable for swimming pools and other wet locations; Excellent workability and slump resistance; Suitable for floors with underfloor heating" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@ardex.co.uk" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "ARDEX X 7 W" (IFCTEXT)
    Name = "CementitiousAdhesives_ARDEXX7W_ARDEXUKLtd" (IFCTEXT)
    NominalHeight = 3. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  xbim_MaterialFunctionAssignment | properties | on 1 type object
    MaterialFunctionAssignment (ifcpropertytablevalue)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Cementitious adhesive" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 3. (IFCLENGTHMEASURE) [MILLI METRE]
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_ARDEXUKLtd_CementitiousAdhesives_ARDEXX7W" (IFCTEXT)
    ManufacturerName = "ARDEX UK Ltd" (IFCTEXT)
    ManufacturerURL = "www.ardex.co.uk" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/ts241hth" (IFCTEXT)
    NBSDescription = "Cementitious adhesives" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-50-00/325" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.ardex.co.uk/Portals/0/productdocs/a2e2c287-8549-47f3-9061-6d1022b9af71-ARDEX%20X%207.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_20_31_02_12" (IFCTEXT)
    Uniclass2015Title = "Cementitious adhesives" (IFCTEXT)
    Uniclass2015Version = "Products v1.7" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    BallPressureHardness = "n/a" (IFCTEXT)
    BulkDensityPowder = "Approximately 1.2 kg/litre" (IFCTEXT)
    Classification = "n/a" (IFCTEXT)
    CompressiveStrength = "After 28 days: 17.9 N/mm²" (IFCTEXT)
    OpenTimeMinimum = "30 minutes" (IFCTEXT)
    SetFinal = "Approximately 18 hrs" (IFCTEXT)
    SetInitial = "Approximately 5 hrs" (IFCTEXT)
    ShelfLife = "12 months" (IFCTEXT)
    SlipResistance = "Slip - less than 0.5 mm" (IFCTEXT)
    TensileAdhesionStrength = "Greater than 1 N/mm² under all test conditions" (IFCTEXT)
    TensileAdhesionStrengthEarly = "n/a" (IFCTEXT)
    TensileBendingStrength = "After 28 days: 6.4 N/mm²" (IFCTEXT)
    UnderflooringHeatingSuitablity = "n/a" (IFCTEXT)
    WeightMortar = "Approximately 1.7kg/litre" (IFCTEXT)
  IFC | properties | on 1 type object
    IfcExportAs = "IfcCoveringType" (IFCTEXT)
    IfcExportType = "USERDEFINED" (IFCTEXT)